**Origination Date:** 07/10/17

**Originator:** iconectiv

### Change Order Number: NANC 524

**Description:** MUMP File Layouts – Near Term

**Functional Backwards Compatible:** Yes

**IMPACT/CHANGE ASSESSMENT**

|  |  |  |
| --- | --- | --- |
| DOC | FRS | IIS |
| Y | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CMIP | GDMO | ASN.1 | NPAC | SOA | LSMS |
| N | N | N | N | N |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| XML | XIS | XSD | NPAC | SOA | LSMS |
| N | N | N | N | N |

**Business Need**

The FRS requirement concerning the layout of the Mass Update Mass Porting (MUMP) file template that can be used to upload MUMP data to be used as input for MUMP jobs is at a high level and does not accurately identify the file layout. This doc-only change order will update the existing FRS requirement concerning the MUMP File to make it more accurate. A related Change Order, NANC 525, will provide a long-term view and requirements for specific MUMP File formats. Also see PIM 107.

**Description of Change:**

Changes detailed below.

**FRS:**

Update requirement **RR3-780** in the FRS.

[snip]

**RR3-780 Mass Update File Upload Capability – Template**

NPAC Low-Tech Interface shall accept file data from a spreadsheet template as input data for a Mass Update request. (previously NANC 444, Req 1)

Note: The accepted formats will be all standard MS-Excel (xlsx).

Note: The file layout will include:

* Header Data:
  + Job Type (valid values: Mass Update, Mass Create, Mass Release, Mass Activate, Mass Disconnect, Create-Activate)
  + SPID (valid NPAC SPID value)
  + Select By (valid value: TN/PB List)
  + Scheduled Date (mm/dd/yyyy hh:mm)
  + Case Number (optional, maximum 10 characters)
  + Job Name (required, maximum 100 characters)
  + Suppress Notification to Initiator SP (valid values: TRUE, FALSE)
  + Suppress Notification to Request SP (valid values: TRUE, FALSE)
  + Suppress Notification to Other SP (valid values: TRUE, FALSE)
* Detail Data: (specific to requested Job Type)
  + One line per TN/TN Range or PB/PB Range
  + TN example: 1112223333 or 1112223333-4444
  + PB example: 1234567 or 1234567-8
  + Update data is Job Type specific, for example, for Mass Update, Mass Create, and Mass Create-Activate, it will include:
    - LRN (optional)
    - LIDB DPC (optional)
    - CNAM DPC (optional)
    - CLASS DPC (optional)
    - ISVM DPC (optional)
    - WSMSC DPC (optional, only if supported by SPID)

[snip]